**CABRI 828 URINAL – MODESTY PANELS**
In Cabrillant laminated safety glass (LSG), comprising 2x 5 mm Float toughened safety glass (ESG) as per EN 12150-2. 1 sheet of glass in centre enamelled over entire surface using screen printing process, 1.52 mm PVB film. Front side with 2 radii of 30 mm. Size 45 x 90 cm.

Wall fixing of urinal modesty panel using two double angle brackets.
No visible screw fittings.

Construction parts:

All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.

Enamelled safety glass:

Enamels are lead- and cadmium-free, 100% recyclable.