**CABRI 603 PARTITION WALLS**
Partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float 10 mm, entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Listral SR 200, 10 mm, (textured surface), entire surface enamelled, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Satinato 10 mm (satin finish on one side), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Partition walls and front walls made of Cabrillant toughened safety glass (ESG) as per EN 12150-2. Float, bright white 10 mm (glass without green cast), entire surface enamelled using screen printing process, all edges polished smooth. Colours as per standard colour range. Glass height     cm.

Partition walls and front walls in Cabrillant laminated safety glass (LSG), comprising 2x 5 mm Float toughened safety glass (ESG) as per EN 12150-2. 1 sheet of glass in centre enamelled over entire surface using screen printing process, 1.52 mm PVB film. Glass height     cm.

Wall fixing with 2 aluminium alloy fasteners. Partition walls fastened to front wall with 2 aluminium alloy
angle brackets. Front wall sits on construction provided by customer using two aluminium alloy feet.

Fixed front parts supported by partition wall feet on ready tiled floor. Floor rosette in solid aluminium. Ground clearance    cm.

Partition walls stabilised by continuous circular tubes at top, 25 mm diameter, incl. materials for fixing to walls.

Construction parts:

All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.

Enamelled safety glass:

Enamels are lead- and cadmium-free, 100% recyclable.