**CABRI 800 PARTITION WALLS**
Doors, partition walls and front walls in laminated safety glass (LSG), comprising 2x 5 mm Float toughened safety glass (ESG) as per EN 12150-2. 1 sheet of glass in centre enamelled over entire surface using screen printing process, 1.52 mm PVB film. Glass height     cm.

Doors open inwards.

Angle brackets used for wall fixing and connection of partition walls with front walls. No visible screw fittings.

Partition walls with partition wall feet stand on ready tiled floor. Floor rosette in solid aluminium.
Ground clearance    cm.

Partition walls stabilised at top by continuous circular tube, recessed, diameter 25 mm.

Fittings

In each cubicle: 2 Aluminium alloy door hinges with stainless
 steel pin and nylon sliding surfaces, incl. integrated spring
 to hold the doors open
 1 Olive lock with internal
 knob and external red/green indicator
 1 Door stop, theft-proof fitting
 1 Screen between
 door hinges on interior
 1 Screen on lock side,
 applied on interior

Alternative: 1 Lock with aluminium handle. External
 red-green indicator, internal rotary olive handle

 All fittings clear anodised, stainless

Construction parts:

All connecting elements in aluminium (DIN 1725) are 100% corrosion-resistant and environmentally friendly. 100% recyclable.

Enamelled safety glass:

Enamels are lead- and cadmium-free, 100% recyclable.