**PARTITION WALLS CABRI 905 floating with invisible fastening**

The partition feet and thestabilizing rod are relegated back-

and give the system a [flush](https://dict.leo.org/englisch-deutsch/flush)-mounted, elegant

and a floating impression.

Fittings outside utilizing invisible point fastening.

Doors, forehead and side walls made of Cabrillant composite safety
glass 15 mm CSG made of 8 + 6 mm float extra-white single-pane
safety glass (ESG)

according to EN 12150-2. Both glasses are enamelled in the middle full-surface,
EVA film 0.8 mm, all edges polished flat.

Partition walls made of Cabrillant laminated safety glass LSG
made of 2 x 5 mm float extra-white single-pane safety glass
(ESG) according to EN 12150-2.
Both glasses in the middle all-surface enamelled,
EVA – foil 0.8 mm, all edges polished flat.

Glass height     cm.

Doors inward - opening.

Wall fastening and connection of the partition walls with the end walls

with cross-fitting and rosettes

including strengthening angle.

Partition wall with partition wall base supported on the

pre-tiled floor. Soil rosette in aluminium solid.

Ground clearance cm.

Stabilization of the partition walls utilizing a run-through,

recessed round tube, diameter 25 mm.

Fittings

per cell: 2 Light metal door bands with Stainless steel axis of

 rotation and Nylon sliding surfaces,

incl. built-in spring
for holding a position of the doors

 1 Olive lock with inner turn knob,
 outside with red-green display

 Housing and cover rosette in V4A
 1 door buffer, theft-proof mounted

 1 clamp screen protection between the door bands on the inside

 1 View protection on the lock side inside

 mounted.

**All fittings colourless anodised, stainless**
construction parts:

All fasteners in aluminium (DIN 1725) are 100%

corrosion-resistant and environmentally friendly.

100% recycling capability.

Enamelled safety glass:

enamel colours lead- and cadmium-free, 100%
recycling possibility.